(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A3")
	(title_block
		(title "left")
		(date "2024-10-01")
		(rev "v0.2")
		(company "Tilman Baumann")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0.05)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "q_bottom")
	(net 2 "C1")
	(net 3 "GND")
	(net 4 "q_home")
	(net 5 "q_top")
	(net 6 "q_num")
	(net 7 "q_f")
	(net 8 "w_bottom")
	(net 9 "C2")
	(net 10 "w_home")
	(net 11 "w_top")
	(net 12 "w_num")
	(net 13 "w_f")
	(net 14 "e_bottom")
	(net 15 "C3")
	(net 16 "e_home")
	(net 17 "e_top")
	(net 18 "e_num")
	(net 19 "e_f")
	(net 20 "r_bottom")
	(net 21 "C4")
	(net 22 "r_home")
	(net 23 "r_top")
	(net 24 "r_num")
	(net 25 "r_f")
	(net 26 "t_bottom")
	(net 27 "C5")
	(net 28 "t_home")
	(net 29 "t_top")
	(net 30 "t_num")
	(net 31 "t_f")
	(net 32 "left_bottom")
	(net 33 "C0")
	(net 34 "left_home")
	(net 35 "left_top")
	(net 36 "left_num")
	(net 37 "left_f")
	(net 38 "enter_bottom")
	(net 39 "C6")
	(net 40 "enter_home")
	(net 41 "enter_top")
	(net 42 "enter_num")
	(net 43 "enter_f")
	(net 44 "one_down")
	(net 45 "one_up")
	(net 46 "two_down")
	(net 47 "two_up")
	(net 48 "three_down")
	(net 49 "three_up")
	(net 50 "space_space")
	(net 51 "R4")
	(net 52 "R3")
	(net 53 "R2")
	(net 54 "R1")
	(net 55 "R0")
	(net 56 "R6")
	(net 57 "R5")
	(net 58 "RAW")
	(net 59 "RST")
	(net 60 "VCC")
	(net 61 "P10")
	(net 62 "DPC")
	(net 63 "DPD")
	(net 64 "DPE")
	(net 65 "R7")
	(net 66 "P101")
	(net 67 "P102")
	(net 68 "P107")
	(net 69 "BAT_P")
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 100 64.5 -90)
		(property "Reference" "D23"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "r_top")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 80.25 115.5 -90)
		(property "Reference" "D41"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "R5")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "three_up")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 117 64.5 -90)
		(property "Reference" "D28"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "t_top")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 27.25 115.5 -90)
		(property "Reference" "D37"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "R5")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "one_up")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 83 64.5 -90)
		(property "Reference" "D18"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "e_top")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 27.25 30.5 -90)
		(property "Reference" "D5"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "R0")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "left_f")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 49 81.5 -90)
		(property "Reference" "D7"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "q_home")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 117 98.5 -90)
		(property "Reference" "D26"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "t_bottom")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 49 30.5 -90)
		(property "Reference" "D10"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "R0")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "q_f")
		)
	)
	(footprint "ceoloide:mcu_nice_nano"
		(layer "F.Cu")
		(at 99.74 13.25 -90)
		(property "Reference" "MCU1"
			(at 0 -15 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "VCC"
			(at -4.47 -5.08 -90)
			(layer "B.SilkS")
		)
		(fp_text user "RAW"
			(at -4.47 -12.7 -90)
			(layer "B.SilkS")
		)
		(fp_text user "R4"
			(at 4.47 7.62 -90)
			(layer "B.SilkS")
		)
		(fp_text user "GND"
			(at -4.47 -10.16 -90)
			(layer "B.SilkS")
		)
		(fp_text user "GND"
			(at 4.47 -7.62 -90)
			(layer "B.SilkS")
		)
		(fp_text user "P10"
			(at -4.47 15.24 -90)
			(layer "B.SilkS")
		)
		(fp_text user "C2"
			(at -4.47 2.54 -90)
			(layer "B.SilkS")
		)
		(fp_text user "DPE"
			(at 4.47 -2.54 -90)
			(layer "B.SilkS")
		)
		(fp_text user "R2"
			(at 4.47 2.54 -90)
			(layer "B.SilkS")
		)
		(fp_text user "R7"
			(at 4.47 15.24 -90)
			(layer "B.SilkS")
		)
		(fp_text user "C3"
			(at -4.47 5.08 -90)
			(layer "B.SilkS")
		)
		(fp_text user "R3"
			(at 4.47 5.08 -90)
			(layer "B.SilkS")
		)
		(fp_text user "C0"
			(at -4.47 -2.54 -90)
			(layer "B.SilkS")
		)
		(fp_text user "C1"
			(at -4.47 0 -90)
			(layer "B.SilkS")
		)
		(fp_text user "C5"
			(at -4.47 10.16 -90)
			(layer "B.SilkS")
		)
		(fp_text user "C6"
			(at -4.47 12.7 -90)
			(layer "B.SilkS")
		)
		(fp_text user "R5"
			(at 4.47 10.16 -90)
			(layer "B.SilkS")
		)
		(fp_text user "R1"
			(at 4.47 0 -90)
			(layer "B.SilkS")
		)
		(fp_text user "C4"
			(at -4.47 7.62 -90)
			(layer "B.SilkS")
		)
		(fp_text user "DPC"
			(at 4.47 -12.7 -90)
			(layer "B.SilkS")
		)
		(fp_text user "GND"
			(at 4.47 -5.08 -90)
			(layer "B.SilkS")
		)
		(fp_text user "RST"
			(at -4.47 -7.62 -90)
			(layer "B.SilkS")
		)
		(fp_text user "DPD"
			(at 4.47 -10.16 -90)
			(layer "B.SilkS")
		)
		(fp_text user "C0"
			(at -4.47 -2.54 -90)
			(layer "F.SilkS")
		)
		(fp_text user "RST"
			(at -4.47 -7.62 -90)
			(layer "F.SilkS")
		)
		(fp_text user "C2"
			(at -4.47 2.54 -90)
			(layer "F.SilkS")
		)
		(fp_text user "R4"
			(at 4.47 7.62 -90)
			(layer "F.SilkS")
		)
		(fp_text user "RAW"
			(at -4.47 -12.7 -90)
			(layer "F.SilkS")
		)
		(fp_text user "C1"
			(at -4.47 0 -90)
			(layer "F.SilkS")
		)
		(fp_text user "R2"
			(at 4.47 2.54 -90)
			(layer "F.SilkS")
		)
		(fp_text user "C4"
			(at -4.47 7.62 -90)
			(layer "F.SilkS")
		)
		(fp_text user "DPC"
			(at 4.47 -12.7 -90)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 4.47 -5.08 -90)
			(layer "F.SilkS")
		)
		(fp_text user "DPD"
			(at 4.47 -10.16 -90)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -4.47 -10.16 -90)
			(layer "F.SilkS")
		)
		(fp_text user "C6"
			(at -4.47 12.7 -90)
			(layer "F.SilkS")
		)
		(fp_text user "R7"
			(at 4.47 15.24 -90)
			(layer "F.SilkS")
		)
		(fp_text user "DPE"
			(at 4.47 -2.54 -90)
			(layer "F.SilkS")
		)
		(fp_text user "VCC"
			(at -4.47 -5.08 -90)
			(layer "F.SilkS")
		)
		(fp_text user "R1"
			(at 4.47 0 -90)
			(layer "F.SilkS")
		)
		(fp_text user "C5"
			(at -4.47 10.16 -90)
			(layer "F.SilkS")
		)
		(fp_text user "R3"
			(at 4.47 5.08 -90)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 4.47 -7.62 -90)
			(layer "F.SilkS")
		)
		(fp_text user "P10"
			(at -4.47 15.24 -90)
			(layer "F.SilkS")
		)
		(fp_text user "R5"
			(at 4.47 10.16 -90)
			(layer "F.SilkS")
		)
		(fp_text user "C3"
			(at -4.47 5.08 -90)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at 7.62 -12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "DPC")
		)
		(pad "2" thru_hole circle
			(at 7.62 -10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "DPD")
		)
		(pad "3" thru_hole circle
			(at 7.62 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "4" thru_hole circle
			(at 7.62 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "5" thru_hole circle
			(at 7.62 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "DPE")
		)
		(pad "6" thru_hole circle
			(at 7.62 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "R1")
		)
		(pad "7" thru_hole circle
			(at 7.62 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "R2")
		)
		(pad "8" thru_hole circle
			(at 7.62 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "R3")
		)
		(pad "9" thru_hole circle
			(at 7.62 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "R4")
		)
		(pad "10" thru_hole circle
			(at 7.62 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "R5")
		)
		(pad "11" thru_hole circle
			(at 7.62 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "R6")
		)
		(pad "12" thru_hole circle
			(at 7.62 15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "R7")
		)
		(pad "13" thru_hole circle
			(at -7.62 15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "P10")
		)
		(pad "14" thru_hole circle
			(at -7.62 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "C6")
		)
		(pad "15" thru_hole circle
			(at -7.62 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "C5")
		)
		(pad "16" thru_hole circle
			(at -7.62 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "C4")
		)
		(pad "17" thru_hole circle
			(at -7.62 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "C3")
		)
		(pad "18" thru_hole circle
			(at -7.62 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "C2")
		)
		(pad "19" thru_hole circle
			(at -7.62 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "C1")
		)
		(pad "20" thru_hole circle
			(at -7.62 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "C0")
		)
		(pad "21" thru_hole circle
			(at -7.62 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "VCC")
		)
		(pad "22" thru_hole circle
			(at -7.62 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "RST")
		)
		(pad "23" thru_hole circle
			(at -7.62 -10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "24" thru_hole circle
			(at -7.62 -12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "RAW")
		)
		(pad "25" thru_hole circle
			(at 5.08 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "P101")
		)
		(pad "26" thru_hole circle
			(at 2.54 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "P102")
		)
		(pad "27" thru_hole circle
			(at 0 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "P107")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 49 47.5 -90)
		(property "Reference" "D9"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "q_num")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 124.5 115.5 -90)
		(property "Reference" "D42"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "R5")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "space_space")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 49 98.5 -90)
		(property "Reference" "D6"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "q_bottom")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 27.25 132.5 -90)
		(property "Reference" "D36"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "R6")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "one_down")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 100 47.5 -90)
		(property "Reference" "D24"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "r_num")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 83 30.5 -90)
		(property "Reference" "D20"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "R0")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "e_f")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 138.75 98.5 -90)
		(property "Reference" "D31"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "enter_bottom")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 100 98.5 -90)
		(property "Reference" "D21"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "r_bottom")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 49 64.5 -90)
		(property "Reference" "D8"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "q_top")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 83 81.5 -90)
		(property "Reference" "D17"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "e_home")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 83 98.5 -90)
		(property "Reference" "D16"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "e_bottom")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 117 81.5 -90)
		(property "Reference" "D27"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "t_home")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 27.25 47.5 -90)
		(property "Reference" "D4"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "left_num")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 53.75 132.5 -90)
		(property "Reference" "D38"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "R6")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "two_down")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 66 98.5 -90)
		(property "Reference" "D11"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "w_bottom")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 27.25 81.5 -90)
		(property "Reference" "D2"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "left_home")
		)
	)
	(footprint "ceoloide:utility_ergogen_logo"
		(layer "F.Cu")
		(at 63.23 13.25)
		(property "Reference" "LOGO1"
			(at 4.572 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
	)
	(footprint "ceoloide:display_nice_view"
		(layer "F.Cu")
		(at 98.24 13.25 -90)
		(property "Reference" "DISP1"
			(at 0 20 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "VCC"
			(at 0.15 14.6 -90)
			(layer "F.SilkS")
		)
		(fp_text user "DA"
			(at -5.08 13.1 -90)
			(layer "F.SilkS")
		)
		(fp_text user "CL"
			(at -2.48 13.1 -90)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 2.62 13.1 -90)
			(layer "F.SilkS")
		)
		(fp_text user "CS"
			(at 5.12 13.1 -90)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole oval
			(at -5.08 16.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "DPE")
		)
		(pad "2" thru_hole oval
			(at -2.54 16.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "3" thru_hole oval
			(at 0 16.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "VCC")
		)
		(pad "4" thru_hole oval
			(at 2.54 16.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "DPC")
		)
		(pad "5" thru_hole circle
			(at 5.08 16.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "DPD")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 83 47.5 -90)
		(property "Reference" "D19"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "e_num")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 138.75 47.5 -90)
		(property "Reference" "D34"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "enter_num")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 66 64.5 -90)
		(property "Reference" "D13"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "w_top")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 53.75 115.5 -90)
		(property "Reference" "D39"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "R5")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "two_up")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 117 47.5 -90)
		(property "Reference" "D29"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "t_num")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 138.75 30.5 -90)
		(property "Reference" "D35"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "R0")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "enter_f")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 66 81.5 -90)
		(property "Reference" "D12"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "w_home")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 138.75 64.5 -90)
		(property "Reference" "D33"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "enter_top")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 66 47.5 -90)
		(property "Reference" "D14"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "w_num")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 80.25 132.5 -90)
		(property "Reference" "D40"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "R6")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "three_down")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 27.25 64.5 -90)
		(property "Reference" "D3"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "left_top")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 100 81.5 -90)
		(property "Reference" "D22"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "r_home")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 100 30.5 -90)
		(property "Reference" "D25"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "R0")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "r_f")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 27.25 98.5 -90)
		(property "Reference" "D1"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "left_bottom")
		)
	)
	(footprint "ceoloide:battery_connector_jst_ph_2"
		(layer "F.Cu")
		(at 76.23 20.25 180)
		(property "Reference" "JST1"
			(at 0 4.8 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 180)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole roundrect
			(at -1 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.2)
			(net 3 "GND")
		)
		(pad "2" thru_hole oval
			(at 1 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "BAT_P")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 66 30.5 -90)
		(property "Reference" "D15"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "R0")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "w_f")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 138.75 81.5 -90)
		(property "Reference" "D32"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "enter_home")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 117 30.5 -90)
		(property "Reference" "D30"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "R0")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "t_f")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 73.75 100)
		(property "Reference" "S6"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "w_bottom")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 90.75 83)
		(property "Reference" "S12"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 16 "e_home")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "C3")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 35 32)
		(property "Reference" "S30"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 37 "left_f")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 33 "C0")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 124.75 66)
		(property "Reference" "S23"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 29 "t_top")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "C5")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 61.5 134)
		(property "Reference" "S38"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 46 "two_down")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 146.5 66)
		(property "Reference" "S33"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 41 "enter_top")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 39 "C6")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 35 117)
		(property "Reference" "S37"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 45 "one_up")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 33 "C0")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 35 134)
		(property "Reference" "S36"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 44 "one_down")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 33 "C0")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 56.75 32)
		(property "Reference" "S5"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 7 "q_f")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 107.75 83)
		(property "Reference" "S17"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 22 "r_home")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "C4")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 73.75 83)
		(property "Reference" "S7"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 10 "w_home")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 35 83)
		(property "Reference" "S27"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 34 "left_home")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 33 "C0")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 107.75 66)
		(property "Reference" "S18"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 23 "r_top")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "C4")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 61.5 117)
		(property "Reference" "S39"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 47 "two_up")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 107.75 32)
		(property "Reference" "S20"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 25 "r_f")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "C4")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 90.75 100)
		(property "Reference" "S11"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 14 "e_bottom")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "C3")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 146.5 32)
		(property "Reference" "S35"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 43 "enter_f")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 39 "C6")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 35 49)
		(property "Reference" "S29"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 36 "left_num")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 33 "C0")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 90.75 49)
		(property "Reference" "S14"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 18 "e_num")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "C3")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 88 117)
		(property "Reference" "S41"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 49 "three_up")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 132.25 117)
		(property "Reference" "S42"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 50 "space_space")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "C4")
		)
	)
	(footprint "ceoloide:reset_switch_tht_top"
		(layer "B.Cu")
		(at 69.23 13.25 90)
		(property "Reference" "RST1"
			(at 0 2.55 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(fp_text user "RST"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(pad "1" thru_hole circle
			(at 3.25 0 90)
			(size 2 2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "RST")
		)
		(pad "2" thru_hole circle
			(at -3.25 0 90)
			(size 2 2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 73.75 32)
		(property "Reference" "S10"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 13 "w_f")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 56.75 49)
		(property "Reference" "S4"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 6 "q_num")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 73.75 49)
		(property "Reference" "S9"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 12 "w_num")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 35 100)
		(property "Reference" "S26"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 32 "left_bottom")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 33 "C0")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 56.75 100)
		(property "Reference" "S1"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "q_bottom")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 107.75 100)
		(property "Reference" "S16"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 20 "r_bottom")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "C4")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 146.5 100)
		(property "Reference" "S31"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 38 "enter_bottom")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 39 "C6")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 107.75 49)
		(property "Reference" "S19"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 24 "r_num")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "C4")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 146.5 49)
		(property "Reference" "S34"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 42 "enter_num")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 39 "C6")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 56.75 66)
		(property "Reference" "S3"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 5 "q_top")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 90.75 66)
		(property "Reference" "S13"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 17 "e_top")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "C3")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 88 134)
		(property "Reference" "S40"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 48 "three_down")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 124.75 100)
		(property "Reference" "S21"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 26 "t_bottom")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "C5")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 56.75 83)
		(property "Reference" "S2"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 4 "q_home")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 146.5 83)
		(property "Reference" "S32"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 40 "enter_home")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 39 "C6")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 73.75 66)
		(property "Reference" "S8"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 11 "w_top")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 124.75 83)
		(property "Reference" "S22"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 28 "t_home")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "C5")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 124.75 32)
		(property "Reference" "S25"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 31 "t_f")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "C5")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 124.75 49)
		(property "Reference" "S24"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 30 "t_num")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "C5")
		)
	)
	(footprint "ceoloide:power_switch_smd_side"
		(layer "B.Cu")
		(at 73.23 4.75 90)
		(property "Reference" "PWR1"
			(at -3.6 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "OFF"
			(at 0 5 90)
			(layer "B.SilkS")
		)
		(fp_text user "PWR1"
			(at -3.5 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "ON"
			(at 0 -5 90)
			(layer "B.SilkS")
		)
		(pad "" smd rect
			(at -1.085 -3.65)
			(size 1 0.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "" smd rect
			(at -1.085 3.65)
			(size 1 0.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0.025 -1.5 180)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0.025 1.5 180)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" smd rect
			(at 1.125 -3.65)
			(size 1 0.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "" smd rect
			(at 1.125 3.65)
			(size 1 0.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "1" smd rect
			(at -1.735 -2.25)
			(size 0.7 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 69 "BAT_P")
		)
		(pad "2" smd rect
			(at -1.735 0.75)
			(size 0.7 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 58 "RAW")
		)
		(pad "3" smd rect
			(at -1.735 2.25)
			(size 0.7 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 90.75 32)
		(property "Reference" "S15"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 19 "e_f")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "C3")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 35 66)
		(property "Reference" "S28"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 35 "left_top")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 33 "C0")
		)
	)
	(gr_line
		(start 159.75 24)
		(end 159.75 125)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 159.25 125.5)
		(end 101.75 125.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 64.865121 2.680832)
		(end 47.865121 23.180832)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 100.75 142.5)
		(end 22.25 142.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 22.25 23.5)
		(end 47.75 23.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 159.75 125)
		(mid 159.603553 125.353553)
		(end 159.25 125.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 101.25 126)
		(mid 101.396447 125.646447)
		(end 101.75 125.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 101.25 142)
		(mid 101.103553 142.353553)
		(end 100.75 142.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 21.75 142)
		(end 21.75 24)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 22.25 142.5)
		(mid 21.896447 142.353553)
		(end 21.75 142)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 47.75 23.5)
		(mid 47.77966 23.330353)
		(end 47.865121 23.180832)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 101.25 126)
		(end 101.25 142)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 64.865121 2.680832)
		(mid 65.037378 2.54746)
		(end 65.25 2.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.25 2.5)
		(end 65.25 2.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 133.75 23.5)
		(end 159.25 23.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 21.75 24)
		(mid 21.896447 23.646447)
		(end 22.25 23.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 133.634879 23.180832)
		(mid 133.72034 23.330353)
		(end 133.75 23.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 133.634879 23.180832)
		(end 116.634879 2.680832)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 159.25 23.5)
		(mid 159.603553 23.646447)
		(end 159.75 24)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 116.25 2.5)
		(mid 116.462622 2.547461)
		(end 116.634879 2.680832)
		(layer "Edge.Cuts")
	)
	(gr_text "https://github.com/tbaumann/typematrix_split_new/"
		(at 132.25 123 0)
		(layer "B.SilkS")
	)
	(gr_text "v0.2"
		(at 61.23 21.25 0)
		(layer "F.SilkS")
	)
	(gr_text "https://github.com/tbaumann/typematrix_split_new/"
		(at 132.25 123 0)
		(layer "F.SilkS")
	)
	(gr_text "JLCJLCJLCJLC"
		(at 132.25 107 0)
		(layer "F.SilkS")
	)
)
