(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A3")
	(title_block
		(title "right")
		(date "2024-10-01")
		(rev "v0.2")
		(company "Tilman Baumann")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0.05)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "mirror_q_bottom")
	(net 2 "C1")
	(net 3 "GND")
	(net 4 "mirror_q_home")
	(net 5 "mirror_q_top")
	(net 6 "mirror_q_num")
	(net 7 "mirror_q_f")
	(net 8 "mirror_w_bottom")
	(net 9 "C2")
	(net 10 "mirror_w_home")
	(net 11 "mirror_w_top")
	(net 12 "mirror_w_num")
	(net 13 "mirror_w_f")
	(net 14 "mirror_e_bottom")
	(net 15 "C3")
	(net 16 "mirror_e_home")
	(net 17 "mirror_e_top")
	(net 18 "mirror_e_num")
	(net 19 "mirror_e_f")
	(net 20 "mirror_r_bottom")
	(net 21 "C4")
	(net 22 "mirror_r_home")
	(net 23 "mirror_r_top")
	(net 24 "mirror_r_num")
	(net 25 "mirror_r_f")
	(net 26 "mirror_t_bottom")
	(net 27 "C5")
	(net 28 "mirror_t_home")
	(net 29 "mirror_t_top")
	(net 30 "mirror_t_num")
	(net 31 "mirror_t_f")
	(net 32 "mirror_one_down")
	(net 33 "C0")
	(net 34 "mirror_one_up")
	(net 35 "mirror_two_down")
	(net 36 "mirror_two_up")
	(net 37 "mirror_three_down")
	(net 38 "mirror_three_up")
	(net 39 "mirror_alt_space")
	(net 40 "mirror_sym_bottom")
	(net 41 "mirror_sym_home")
	(net 42 "mirror_sym_top")
	(net 43 "mirror_sym_num")
	(net 44 "mirror_sym_f")
	(net 45 "mirror_enter_bottom")
	(net 46 "C6")
	(net 47 "mirror_enter_home")
	(net 48 "mirror_enter_top")
	(net 49 "mirror_enter_num")
	(net 50 "mirror_enter_f")
	(net 51 "mirror_sym_ctl_down")
	(net 52 "C7")
	(net 53 "mirror_sym_ctl_up")
	(net 54 "mirror_space_space")
	(net 55 "R4")
	(net 56 "R3")
	(net 57 "R2")
	(net 58 "R1")
	(net 59 "R0")
	(net 60 "R6")
	(net 61 "R5")
	(net 62 "RAW")
	(net 63 "RST")
	(net 64 "VCC")
	(net 65 "P10")
	(net 66 "DPC")
	(net 67 "DPD")
	(net 68 "DPE")
	(net 69 "R7")
	(net 70 "P101")
	(net 71 "P102")
	(net 72 "P107")
	(net 73 "BAT_P")
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 361 81.5 90)
		(property "Reference" "D40"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "mirror_sym_home")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 254.25 47.5 90)
		(property "Reference" "D29"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "mirror_enter_num")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 268.5 115.5 90)
		(property "Reference" "D38"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "R5")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "mirror_space_space")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 327 98.5 90)
		(property "Reference" "D6"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "mirror_w_bottom")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 293 64.5 90)
		(property "Reference" "D18"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "mirror_r_top")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 293 81.5 90)
		(property "Reference" "D17"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "mirror_r_home")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 310 47.5 90)
		(property "Reference" "D14"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "mirror_e_num")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 382.75 132.5 90)
		(property "Reference" "D44"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "R6")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "mirror_sym_ctl_down")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 327 115.5 90)
		(property "Reference" "D36"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "R5")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "mirror_three_up")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 310 98.5 90)
		(property "Reference" "D11"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "mirror_e_bottom")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 382.75 30.5 90)
		(property "Reference" "D50"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "R0")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "mirror_sym_f")
		)
	)
	(footprint "ceoloide:display_nice_view"
		(layer "F.Cu")
		(at 294.76 13.25 90)
		(property "Reference" "DISP1"
			(at 0 20 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "DA"
			(at -5.08 13.1 90)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 2.62 13.1 90)
			(layer "F.SilkS")
		)
		(fp_text user "VCC"
			(at 0.15 14.6 90)
			(layer "F.SilkS")
		)
		(fp_text user "CS"
			(at 5.12 13.1 90)
			(layer "F.SilkS")
		)
		(fp_text user "CL"
			(at -2.48 13.1 90)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole oval
			(at -5.08 16.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "DPE")
		)
		(pad "2" thru_hole oval
			(at -2.54 16.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "3" thru_hole oval
			(at 0 16.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "VCC")
		)
		(pad "4" thru_hole oval
			(at 2.54 16.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "DPC")
		)
		(pad "5" thru_hole circle
			(at 5.08 16.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "DPD")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 382.75 47.5 90)
		(property "Reference" "D49"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "mirror_sym_num")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 254.25 98.5 90)
		(property "Reference" "D26"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "mirror_enter_bottom")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 382.75 64.5 90)
		(property "Reference" "D48"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "mirror_sym_top")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 361 30.5 90)
		(property "Reference" "D43"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "R0")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "mirror_sym_f")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 310 64.5 90)
		(property "Reference" "D13"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "mirror_e_top")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 310 81.5 90)
		(property "Reference" "D12"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "mirror_e_home")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 344 47.5 90)
		(property "Reference" "D4"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "mirror_q_num")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 276 30.5 90)
		(property "Reference" "D25"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "R0")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "mirror_t_f")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 382.75 81.5 90)
		(property "Reference" "D47"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "mirror_sym_home")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 344 64.5 90)
		(property "Reference" "D3"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "mirror_q_top")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 361 98.5 90)
		(property "Reference" "D39"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "mirror_sym_bottom")
		)
	)
	(footprint "ceoloide:mcu_nice_nano"
		(layer "F.Cu")
		(at 293.26 13.25 90)
		(property "Reference" "MCU1"
			(at 0 -15 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "C1"
			(at -4.47 0 90)
			(layer "B.SilkS")
		)
		(fp_text user "C3"
			(at -4.47 5.08 90)
			(layer "B.SilkS")
		)
		(fp_text user "C6"
			(at -4.47 12.7 90)
			(layer "B.SilkS")
		)
		(fp_text user "VCC"
			(at -4.47 -5.08 90)
			(layer "B.SilkS")
		)
		(fp_text user "GND"
			(at -4.47 -10.16 90)
			(layer "B.SilkS")
		)
		(fp_text user "GND"
			(at 4.47 -7.62 90)
			(layer "B.SilkS")
		)
		(fp_text user "DPD"
			(at 4.47 -10.16 90)
			(layer "B.SilkS")
		)
		(fp_text user "R4"
			(at 4.47 7.62 90)
			(layer "B.SilkS")
		)
		(fp_text user "C2"
			(at -4.47 2.54 90)
			(layer "B.SilkS")
		)
		(fp_text user "R2"
			(at 4.47 2.54 90)
			(layer "B.SilkS")
		)
		(fp_text user "C4"
			(at -4.47 7.62 90)
			(layer "B.SilkS")
		)
		(fp_text user "C5"
			(at -4.47 10.16 90)
			(layer "B.SilkS")
		)
		(fp_text user "R3"
			(at 4.47 5.08 90)
			(layer "B.SilkS")
		)
		(fp_text user "GND"
			(at 4.47 -5.08 90)
			(layer "B.SilkS")
		)
		(fp_text user "R5"
			(at 4.47 10.16 90)
			(layer "B.SilkS")
		)
		(fp_text user "RST"
			(at -4.47 -7.62 90)
			(layer "B.SilkS")
		)
		(fp_text user "R1"
			(at 4.47 0 90)
			(layer "B.SilkS")
		)
		(fp_text user "C0"
			(at -4.47 -2.54 90)
			(layer "B.SilkS")
		)
		(fp_text user "DPC"
			(at 4.47 -12.7 90)
			(layer "B.SilkS")
		)
		(fp_text user "P10"
			(at -4.47 15.24 90)
			(layer "B.SilkS")
		)
		(fp_text user "RAW"
			(at -4.47 -12.7 90)
			(layer "B.SilkS")
		)
		(fp_text user "R7"
			(at 4.47 15.24 90)
			(layer "B.SilkS")
		)
		(fp_text user "DPE"
			(at 4.47 -2.54 90)
			(layer "B.SilkS")
		)
		(fp_text user "DPE"
			(at 4.47 -2.54 90)
			(layer "F.SilkS")
		)
		(fp_text user "VCC"
			(at -4.47 -5.08 90)
			(layer "F.SilkS")
		)
		(fp_text user "RAW"
			(at -4.47 -12.7 90)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 4.47 -5.08 90)
			(layer "F.SilkS")
		)
		(fp_text user "DPD"
			(at 4.47 -10.16 90)
			(layer "F.SilkS")
		)
		(fp_text user "R3"
			(at 4.47 5.08 90)
			(layer "F.SilkS")
		)
		(fp_text user "C3"
			(at -4.47 5.08 90)
			(layer "F.SilkS")
		)
		(fp_text user "DPC"
			(at 4.47 -12.7 90)
			(layer "F.SilkS")
		)
		(fp_text user "R7"
			(at 4.47 15.24 90)
			(layer "F.SilkS")
		)
		(fp_text user "C2"
			(at -4.47 2.54 90)
			(layer "F.SilkS")
		)
		(fp_text user "C1"
			(at -4.47 0 90)
			(layer "F.SilkS")
		)
		(fp_text user "R1"
			(at 4.47 0 90)
			(layer "F.SilkS")
		)
		(fp_text user "C6"
			(at -4.47 12.7 90)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -4.47 -10.16 90)
			(layer "F.SilkS")
		)
		(fp_text user "C5"
			(at -4.47 10.16 90)
			(layer "F.SilkS")
		)
		(fp_text user "R5"
			(at 4.47 10.16 90)
			(layer "F.SilkS")
		)
		(fp_text user "C4"
			(at -4.47 7.62 90)
			(layer "F.SilkS")
		)
		(fp_text user "R4"
			(at 4.47 7.62 90)
			(layer "F.SilkS")
		)
		(fp_text user "RST"
			(at -4.47 -7.62 90)
			(layer "F.SilkS")
		)
		(fp_text user "C0"
			(at -4.47 -2.54 90)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 4.47 -7.62 90)
			(layer "F.SilkS")
		)
		(fp_text user "R2"
			(at 4.47 2.54 90)
			(layer "F.SilkS")
		)
		(fp_text user "P10"
			(at -4.47 15.24 90)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at 7.62 -12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "DPC")
		)
		(pad "2" thru_hole circle
			(at 7.62 -10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "DPD")
		)
		(pad "3" thru_hole circle
			(at 7.62 -7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "4" thru_hole circle
			(at 7.62 -5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "5" thru_hole circle
			(at 7.62 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "DPE")
		)
		(pad "6" thru_hole circle
			(at 7.62 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "R1")
		)
		(pad "7" thru_hole circle
			(at 7.62 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "R2")
		)
		(pad "8" thru_hole circle
			(at 7.62 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "R3")
		)
		(pad "9" thru_hole circle
			(at 7.62 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "R4")
		)
		(pad "10" thru_hole circle
			(at 7.62 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "R5")
		)
		(pad "11" thru_hole circle
			(at 7.62 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "R6")
		)
		(pad "12" thru_hole circle
			(at 7.62 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "R7")
		)
		(pad "13" thru_hole circle
			(at -7.62 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "P10")
		)
		(pad "14" thru_hole circle
			(at -7.62 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "C6")
		)
		(pad "15" thru_hole circle
			(at -7.62 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "C5")
		)
		(pad "16" thru_hole circle
			(at -7.62 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "C4")
		)
		(pad "17" thru_hole circle
			(at -7.62 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "C3")
		)
		(pad "18" thru_hole circle
			(at -7.62 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "C2")
		)
		(pad "19" thru_hole circle
			(at -7.62 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "C1")
		)
		(pad "20" thru_hole circle
			(at -7.62 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "C0")
		)
		(pad "21" thru_hole circle
			(at -7.62 -5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "VCC")
		)
		(pad "22" thru_hole circle
			(at -7.62 -7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "RST")
		)
		(pad "23" thru_hole circle
			(at -7.62 -10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "24" thru_hole circle
			(at -7.62 -12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "RAW")
		)
		(pad "25" thru_hole circle
			(at 5.08 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "P101")
		)
		(pad "26" thru_hole circle
			(at 2.54 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "P102")
		)
		(pad "27" thru_hole circle
			(at 0 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "P107")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 327 81.5 90)
		(property "Reference" "D7"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "mirror_w_home")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 327 30.5 90)
		(property "Reference" "D10"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "R0")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "mirror_w_f")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 361 115.5 90)
		(property "Reference" "D32"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "R5")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "mirror_one_up")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 276 81.5 90)
		(property "Reference" "D22"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "mirror_t_home")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 254.25 81.5 90)
		(property "Reference" "D27"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "mirror_enter_home")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 293 47.5 90)
		(property "Reference" "D19"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "mirror_r_num")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 310 115.5 90)
		(property "Reference" "D37"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "R5")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "mirror_alt_space")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 327 132.5 90)
		(property "Reference" "D35"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "R6")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "mirror_three_down")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 276 64.5 90)
		(property "Reference" "D23"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "mirror_t_top")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 310 30.5 90)
		(property "Reference" "D15"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "R0")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "mirror_e_f")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 327 64.5 90)
		(property "Reference" "D8"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "mirror_w_top")
		)
	)
	(footprint "ceoloide:utility_ergogen_logo"
		(layer "F.Cu")
		(at 329.77 13.25)
		(property "Reference" "LOGO1"
			(at 4.572 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 344 81.5 90)
		(property "Reference" "D2"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "R3")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "mirror_q_home")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 293 98.5 90)
		(property "Reference" "D16"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "mirror_r_bottom")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 344 30.5 90)
		(property "Reference" "D5"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "R0")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "mirror_q_f")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 382.75 98.5 90)
		(property "Reference" "D46"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "mirror_sym_bottom")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 344 98.5 90)
		(property "Reference" "D1"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "mirror_q_bottom")
		)
	)
	(footprint "ceoloide:battery_connector_jst_ph_2"
		(layer "F.Cu")
		(at 316.77 20.25 180)
		(property "Reference" "JST1"
			(at 0 4.8 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 180)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole roundrect
			(at -1 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.2)
			(net 3 "GND")
		)
		(pad "2" thru_hole oval
			(at 1 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "BAT_P")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 276 47.5 90)
		(property "Reference" "D24"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "mirror_t_num")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 254.25 30.5 90)
		(property "Reference" "D30"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "R0")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "mirror_enter_f")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 361 47.5 90)
		(property "Reference" "D42"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "mirror_sym_num")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 344 115.5 90)
		(property "Reference" "D34"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "R5")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "mirror_two_up")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 327 47.5 90)
		(property "Reference" "D9"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "R1")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "mirror_w_num")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 344 132.5 90)
		(property "Reference" "D33"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "R6")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "mirror_two_down")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 254.25 64.5 90)
		(property "Reference" "D28"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "mirror_enter_top")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 361 132.5 90)
		(property "Reference" "D31"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "R6")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "mirror_one_down")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 276 98.5 90)
		(property "Reference" "D21"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "R4")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "mirror_t_bottom")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 382.75 115.5 90)
		(property "Reference" "D45"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "R5")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "mirror_sym_ctl_up")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 361 64.5 90)
		(property "Reference" "D41"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "R2")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "mirror_sym_top")
		)
	)
	(footprint "ceoloide:diode_tht_sod123"
		(layer "F.Cu")
		(at 293 30.5 90)
		(property "Reference" "D20"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "R0")
		)
		(pad "2" smd rect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "mirror_r_f")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 353.25 83)
		(property "Reference" "S34"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 41 "mirror_sym_home")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 33 "C0")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 336.25 49)
		(property "Reference" "S4"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 6 "mirror_q_num")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 246.5 100)
		(property "Reference" "S38"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 45 "mirror_enter_bottom")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 46 "C6")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 319.25 32)
		(property "Reference" "S10"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 13 "mirror_w_f")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 246.5 66)
		(property "Reference" "S40"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 48 "mirror_enter_top")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 46 "C6")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 319.25 66)
		(property "Reference" "S8"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 11 "mirror_w_top")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 353.25 66)
		(property "Reference" "S35"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 42 "mirror_sym_top")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 33 "C0")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 336.25 66)
		(property "Reference" "S3"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 5 "mirror_q_top")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 336.25 32)
		(property "Reference" "S5"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 7 "mirror_q_f")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 375 83)
		(property "Reference" "S46"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 41 "mirror_sym_home")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 52 "C7")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 285.25 66)
		(property "Reference" "S18"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 23 "mirror_r_top")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "C4")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 302.25 66)
		(property "Reference" "S13"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 17 "mirror_e_top")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "C3")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 268.25 66)
		(property "Reference" "S23"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 29 "mirror_t_top")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "C5")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 353.25 32)
		(property "Reference" "S37"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 44 "mirror_sym_f")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 33 "C0")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 302.25 83)
		(property "Reference" "S12"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 16 "mirror_e_home")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "C3")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 302.25 100)
		(property "Reference" "S11"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 14 "mirror_e_bottom")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "C3")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 375 100)
		(property "Reference" "S45"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 40 "mirror_sym_bottom")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 52 "C7")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 319.25 49)
		(property "Reference" "S9"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 12 "mirror_w_num")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 268.25 100)
		(property "Reference" "S21"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 26 "mirror_t_bottom")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "C5")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 268.25 83)
		(property "Reference" "S22"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 28 "mirror_t_home")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "C5")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 375 32)
		(property "Reference" "S49"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 44 "mirror_sym_f")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 52 "C7")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 336.25 83)
		(property "Reference" "S2"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 4 "mirror_q_home")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 375 66)
		(property "Reference" "S47"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 42 "mirror_sym_top")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 52 "C7")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 246.5 83)
		(property "Reference" "S39"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 47 "mirror_enter_home")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 46 "C6")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 319.25 134)
		(property "Reference" "S30"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 37 "mirror_three_down")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 336.25 134)
		(property "Reference" "S28"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 35 "mirror_two_down")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:reset_switch_tht_top"
		(layer "B.Cu")
		(at 323.77 13.25 -90)
		(property "Reference" "RST1"
			(at 0 2.55 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(fp_text user "RST"
			(at 0 0 -90)
			(layer "B.SilkS")
		)
		(pad "1" thru_hole circle
			(at 3.25 0 270)
			(size 2 2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "RST")
		)
		(pad "2" thru_hole circle
			(at -3.25 0 270)
			(size 2 2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 268.25 49)
		(property "Reference" "S24"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 30 "mirror_t_num")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "C5")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 353.25 100)
		(property "Reference" "S33"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 40 "mirror_sym_bottom")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 33 "C0")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 246.5 49)
		(property "Reference" "S41"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 49 "mirror_enter_num")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 46 "C6")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 336.25 117)
		(property "Reference" "S29"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 36 "mirror_two_up")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 375 117)
		(property "Reference" "S44"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 53 "mirror_sym_ctl_up")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 52 "C7")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 319.25 100)
		(property "Reference" "S6"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "mirror_w_bottom")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 285.25 49)
		(property "Reference" "S19"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 24 "mirror_r_num")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "C4")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 319.25 83)
		(property "Reference" "S7"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 10 "mirror_w_home")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 336.25 100)
		(property "Reference" "S1"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "mirror_q_bottom")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "C1")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 268.25 32)
		(property "Reference" "S25"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 31 "mirror_t_f")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "C5")
		)
	)
	(footprint "ceoloide:power_switch_smd_side"
		(layer "B.Cu")
		(at 319.77 4.75 90)
		(property "Reference" "PWR1"
			(at -3.6 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "OFF"
			(at 0 5 90)
			(layer "B.SilkS")
		)
		(fp_text user "ON"
			(at 0 -5 90)
			(layer "B.SilkS")
		)
		(fp_text user "PWR1"
			(at -3.5 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(pad "" smd rect
			(at -1.085 -3.65)
			(size 1 0.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "" smd rect
			(at -1.085 3.65)
			(size 1 0.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0.025 -1.5 180)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0.025 1.5 180)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" smd rect
			(at 1.125 -3.65)
			(size 1 0.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "" smd rect
			(at 1.125 3.65)
			(size 1 0.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "1" smd rect
			(at -1.735 -2.25)
			(size 0.7 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 73 "BAT_P")
		)
		(pad "2" smd rect
			(at -1.735 0.75)
			(size 0.7 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 62 "RAW")
		)
		(pad "3" smd rect
			(at -1.735 2.25)
			(size 0.7 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 375 134)
		(property "Reference" "S43"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 51 "mirror_sym_ctl_down")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 52 "C7")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 375 49)
		(property "Reference" "S48"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 43 "mirror_sym_num")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 52 "C7")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 260.75 117)
		(property "Reference" "S50"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 54 "mirror_space_space")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "C4")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 319.25 117)
		(property "Reference" "S31"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 38 "mirror_three_up")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "C2")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 302.25 49)
		(property "Reference" "S14"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 18 "mirror_e_num")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "C3")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 285.25 32)
		(property "Reference" "S20"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 25 "mirror_r_f")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "C4")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 353.25 117)
		(property "Reference" "S27"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 34 "mirror_one_up")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 33 "C0")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 285.25 100)
		(property "Reference" "S16"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 20 "mirror_r_bottom")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "C4")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 302.25 117)
		(property "Reference" "S32"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 39 "mirror_alt_space")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "C3")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 302.25 32)
		(property "Reference" "S15"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 19 "mirror_e_f")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "C3")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 353.25 49)
		(property "Reference" "S36"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 43 "mirror_sym_num")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 33 "C0")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 246.5 32)
		(property "Reference" "S42"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 50 "mirror_enter_f")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 46 "C6")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 353.25 134)
		(property "Reference" "S26"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 32 "mirror_one_down")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 33 "C0")
		)
	)
	(footprint "ceoloide:switch_choc_v1_v2"
		(layer "B.Cu")
		(at 285.25 83)
		(property "Reference" "S17"
			(at 0 8.8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "" np_thru_hole circle
			(at -5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5.95)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.4 3.4)
			(drill 3.4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 -3.75 195)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5.5 0)
			(size 1.9 1.9)
			(drill 1.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.275 -5.95)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 22 "mirror_r_home")
		)
		(pad "2" smd rect
			(at 8.275 -3.75)
			(size 2.6 2.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "C4")
		)
	)
	(gr_arc
		(start 310.25 125.5)
		(mid 310.603553 125.646447)
		(end 310.75 126)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 258.865121 23.180832)
		(end 275.865121 2.680832)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 258.75 23.5)
		(mid 258.77966 23.330353)
		(end 258.865121 23.180832)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 275.865121 2.680832)
		(mid 276.037378 2.54746)
		(end 276.25 2.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 233.25 24)
		(end 233.25 125)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 388.25 142)
		(end 388.25 24)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 310.75 126)
		(end 310.75 142)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 311.25 142.5)
		(end 387.75 142.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 258.75 23.5)
		(end 233.75 23.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 388.25 142)
		(mid 388.103553 142.353553)
		(end 387.75 142.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 387.75 23.5)
		(mid 388.103553 23.646447)
		(end 388.25 24)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 233.75 125.5)
		(mid 233.396447 125.353553)
		(end 233.25 125)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 344.25 2.5)
		(mid 344.462622 2.547461)
		(end 344.634879 2.680832)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 361.634879 23.180832)
		(mid 361.72034 23.330353)
		(end 361.75 23.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 387.75 23.5)
		(end 361.75 23.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 276.25 2.5)
		(end 344.25 2.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 344.634879 2.680832)
		(end 361.634879 23.180832)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 233.75 125.5)
		(end 310.25 125.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 311.25 142.5)
		(mid 310.896447 142.353553)
		(end 310.75 142)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 233.25 24)
		(mid 233.396447 23.646447)
		(end 233.75 23.5)
		(layer "Edge.Cuts")
	)
	(gr_text "https://github.com/tbaumann/typematrix_split_new/"
		(at 260.75 123 0)
		(layer "B.SilkS")
	)
	(gr_text "JLCJLCJLCJLC"
		(at 260.75 107 0)
		(layer "F.SilkS")
	)
	(gr_text "https://github.com/tbaumann/typematrix_split_new/"
		(at 260.75 123 0)
		(layer "F.SilkS")
	)
	(gr_text "v0.2"
		(at 331.77 21.25 0)
		(layer "F.SilkS")
	)
)
